

|  |  |
| --- | --- |
| **Software Version:** | 1.4.10 |
| **Prom Code Version:** | 2.11.0 |
| **Published Date:** | 2013/05/07 |

**Content:**

[Revision History and System Requirement: 2](#_Toc228273642)

[New Features: 2](#_Toc228273646)

[Problems Fixed: 3](#_Toc228273649)

[Known Issues: 3](#_Toc228273650)

[Related Documentation: 3](#_Toc219089682)

# Revision History and System Requirement:

|  |  |  |  |
| --- | --- | --- | --- |
| **Firmware Version** | **Date** | **Model** | **Hardware Version** |
| V1.4.10 | 2013/05/07 | DCS-100/210/220/230 | N/A |

# New Features:

|  |  |
| --- | --- |
| **Firmware Version** | **New Features** |
| 1.4.10 | 1. Add new camera: DCS-3010/2136L/5010L   Note: DCS-5010L is certificated by DCS-5020L v1.00 |

# Problems Fixed:

|  |  |
| --- | --- |
| **Firmware Version** | **Problems Fixed** |
| 1.4.10 | 1. Fixed the bug that DVC would close unexpectedly during endurance test. ([DBG13040187](javascript:edt('DFKLMFJGAF'))) |
| 1.4.10 | 1. Fixed the bug that DVC would be closed unexpectedly when connect the DUT by 10 sessions ([DBG13040084](javascript:edt('JLBREKKLDP'))) |
| 1.4.10 | 1. DCS-6513 (v0.00.01): DUT isn't PTZ camera model but the PTZ panel is active in DVC. ([DBG13030044](http://tsvportal.dlink.com.tw/dlb_Default.asp?Default_ForSystem=4&Fun=dlb_Bug&sno=DFGKBDHMMD)) |
| 1.4.10 | 1. DCS-6513 (v0.00.01): DUT only have 1 digital input but DVC show 2 digital input. ([DBG13030045](http://tsvportal.dlink.com.tw/dlb_Default.asp?Default_ForSystem=4&Fun=dlb_Bug&sno=GIANBGMPHH)) |
| 1.4.10 | 1. DCS-942L: No enable talk on D-Viewcam |
| 1.4.10 | 1. DCS-6210 (v1.00.06): The maximum bit rate on the DUT would be different from the web UI |
| 1.4.10 | 1. DCS-6513 (v0.00.01): Modify DUT resolution to 800X600 failed, the resolution become 1024X768 |
| 1.4.10 | 1. DCS-6513 (v0.00.01): Modify DUT format/resolution to MPEG4/1024X768 failed, the resolution still is 1600X1200 |

# Known Issues:

|  |  |
| --- | --- |
| **Firmware Version** | **Known Issues** |
| 1.4.10 | 1. DCS-3010 (v1.00.05): no support talk function |
| 1.4.10 | 1. DCS-3010 (v1.00.05): it will have video lag when bitrate is high |
| 1.4.10 | 1. DCS-3010 (v1.00.05): Camera is easy to crash |
| 1.4.10 | 1. DCS-3010 (v1.00.05): Motion Detection function is not stable |

# Related Documentation:

N/A

# Note: