

|  |  |
| --- | --- |
| **Software Version:** | 1.4.6 |
| **Prom Code Version:** |  |
| **Published Date:** | 2012/12/28 |

**Content:**

[Revision History and System Requirement: 2](#_Toc228273642)

[New Features: 2](#_Toc228273646)

[Problems Fixed: 3](#_Toc228273649)

[Known Issues: 3](#_Toc228273650)

[Related Documentation: 3](#_Toc219089682)

# Revision History and System Requirement:

|  |  |  |  |
| --- | --- | --- | --- |
| **Firmware Version** | **Date** | **Model** | **Hardware Version** |
| V1.4.6 | 2012/12/28 | DCS-100/210/220/230 | N/A |

# New Features:

|  |  |
| --- | --- |
| **Firmware Version** | **New Features** |
| 1.4.6 | 1. Add new camera: DCS-931L/933L/6513/6314 2. Firmware upgrade: DCS-6915/2132L/2130L/7513 3. Remove DCS-3713 from support list |

# Problems Fixed:

|  |  |
| --- | --- |
| **Firmware Version** | **Problems Fixed** |
| 1.4.6 | 1. The SetupTool.exe file description should be DevicePack not D-ViewCam. ([DBG12070111](javascript:edt('GICGIONGNG'))) |
| 1.4.6 | 1. Drop audio packet over 16000Kbps |

# Known Issues:

|  |  |
| --- | --- |
| **Firmware Version** | **Known Issues** |
| 1.4.6 | 1. DCS-3010 (V0.2.99\_121014) is not tested by NUUO. Only add model name for vender testing. |
| 1.4.6 | 1. DCS-6915 (dl20121002NSA v1.00.00):Change parameter or Stream Profile will update Audio Codec to 32K |
| 1.4.6 | 1. DCS-6915 (dl20121002NSA v1.00.00): change Resolution and Bitrate to maximum，Live View will delay and break image |
| 1.4.6 | 1. DCS-6915 (dl20121002NSA v1.00.00): Motion detection and IO can only trigger once when camera connects to DVC |
| 1.4.6 | 1. DCS-6915 (dl20121002NSA v1.00.00): Do not support G.726 audio codec |
| 1.4.6 | 1. DCS-6915 (dl20121002NSA v1.00.00): Supports CBR only, the quality setting in DVC would be grayed out. |
| 1.4.6 | 1. DCS-6915 (dl20121002NSA v1.00.00): No support audio talk |
| 1.4.6 | 1. DCS-6513 (v0.00.01): Preset01 will be overlay by Preset02, so it cannot support Patrol01 |
| 1.4.6 | 1. DCS-6513 (v0.00.01): sampleRate should set to 8100 if user want to enable talk |
| 1.4.6 | 1. DCS-3112 (v1.10.02): Preset01 will be overlay by Preset02, so it cannot support Patrol01 |

# Related Documentation:

N/A

# Note:

# HW Support List for Device Pack 1.4.6:

