

|  |  |
| --- | --- |
| **Software Version:** | 1.4.7 |
| **Prom Code Version:** |  |
| **Published Date:** | 2013/05/16 |

**Content:**

[Revision History and System Requirement: 2](#_Toc228273642)

[New Features: 2](#_Toc228273646)

[Problems Fixed: 3](#_Toc228273649)

[Known Issues: 3](#_Toc228273650)

[Related Documentation: 3](#_Toc219089682)

# Revision History and System Requirement:

|  |  |  |  |
| --- | --- | --- | --- |
| **Firmware Version** | **Date** | **Model** | **Hardware Version** |
| V1.4.7 | 2013/03/01 | DCS-100/210/220/230 | N/A |

# New Features:

|  |  |
| --- | --- |
| **Firmware Version** | **New Features** |
| 1.4.7 | 1. Add new camera: DCS-5020L 2. Firmware upgrade: DCS-932L/6210/6511/7413 |

# Problems Fixed:

|  |  |
| --- | --- |
| **Firmware Version** | **Problems Fixed** |
| 1.4.7 | DCS-6112(V)/6113(V) no enable talk issue |
| 1.4.7 | DCS-7413: 30 FPS is available to change in DUT when resolution is 1920X1080 (DBG12100435) |
| 1.4.7 | DCS-6511: Disable then enable speaker/microphone by DVC would change DUT audio in gain level/audio out volume level to 26dB/1 (DBG12080269) |
| 1.4.7 | DCS-6210: DUT disable flip/mirror with image default settings in the webpage but it is enabled in DVC (DBG12100155) |
| 1.4.7 | DCS-6210: The maximum bit rate on the DUT would be different from the web UI ([DBG12110308](javascript:edt('GILKLNLIAH'))) |
|  |  |

# Known Issues:

|  |  |
| --- | --- |
| **Firmware Version** | **Known Issues** |
| 1.4.7 | 1. No support 11025Hz sample rate audio codec of DCS-931L/933L/5020L |
|  |  |

# Related Documentation:

N/A

# Note:

# Camera Support List:

|  |  |  |  |
| --- | --- | --- | --- |
| No. | Device  Name | Final FW | Final HW |
| 1 | DCS-910 | 1.04\_build\_5 | A1G |
| 2 | DCS-920 | 1.04\_build\_5 | A1G |
| 3 | DCS-930 | 1.00 build 2 | A1 |
| 4 | DCS-930L | 1.00 build 2 | A1 |
| 5 | DCS-932 | 1.00 | A1 |
| 6 | DCS-932L | 1.05 | A1 |
| 7 | DCS-933L | 1.00 | A1 |
| 8 | DCS-931L | 1.00 | A1 |
| 9 | DCS-940L | 1 | A1 |
| 10 | DCS-942L | 1 | A1 |
| 11 | DCS-1100 | 1.02\_3522 | A1 |
| 12 | DCS-1100L | 1.03\_4130 | A1 |
| 13 | DCS-1130 | 1.02\_3522 | A1 |
| 14 | DCS-1130L | 1.03\_4130 | A1 |
| 15 | DCS-2102 | 1.04\_3227 | A1 |
| 16 | DCS-2103 |  | A1 |
| 17 | DCS-2210 | 0.02.00 | A1 |
| 18 | DCS-2120 | 1.04\_3227 | A2 |
| 19 | DCS-2120(TW) | 2.01tw | B1 |
| 20 | DCS-2121 | 1.04\_3227 | A1 |
| 21 | DCS-2130 |  | A1 |
| 22 | DCS-2132L | 0.01.02 | A1 |
| 23 | DCS-2230 | 0.02.00 | A1 |
| 24 | DCS-2310L | 1.00.03 | A1 |
| 25 | DCS-2332L | 1.00.03 | A1 |
| 26 | DCS-3010 | 0.01.00 | A1 |
| 27 | DCS-3110 | 1.02 | A2 |
| 28 | DCS-3112 |  | A1 |
| 29 | DCS-3410 | 1.01\_2812 | A2 |
| 30 | DCS-3411 | 1.02\_4125 | A3 |
| 31 | DCS-3415 | 1.00 | A2 |
| 32 | DCS-3420 | 1.03 | A2 |
| 33 | DCS-3430 | 1.02\_4125 | A3 |
| 34 | DCS-3710 | 1.00 | A1 |
| 35 | DCS-3710 B1 | 0.02.00 | B1 |
| 36 | DCS-3713 |  | A1 |
| 37 | DCS-3715 | v1.20\_24\_Aug\_2012 | A1 |
| 38 | DCS-3716 |  | A1 |
| 39 | DCS-5020L | 1.00 | A1 |
| 40 | DCS-5211L | 1.00\_1217\_eu(41024224) | A1 |
| 41 | DCS-5220Ax | 1.05 | A2 |
| 42 | DCS-5220Bx | 2.00 | B1 |
| 43 | DCS-5220(TW) | 2.00tw | A2 |
| 44 | DCS-5222L | 1.00\_1217\_eu(41024224) | A1 |
| 45 | DCS-5230 | 1.02\_4317 | A1 |
| 46 | DCS-5230L | 1.02\_4317 | A1 |
| 47 | DCS-5300 | 1.06 | A3 |
| 48 | DCS-5300G | 2.05 | B2 |
| 49 | DCS-5605 | 1.01\_4126 | A1 |
| 50 | DCS-5610 | 1.01 | A1 |
| 51 | DCS-5635 | 1.01\_4126 | A1 |
| 52 | DCS-6010L | 0.01.13 | A1 |
| 53 | DCS-6110 | 1.00 | A2 |
| 54 | DCS-6112 | 1.2\_6\_Mar 2012 | A1 |
| 55 | DCS-6113 | 1.2\_6\_Mar 2012 | A1 |
| 56 | DCS-6112V | 1.2\_6\_Mar 2012 | A1 |
| 57 | DCS-6113V | 1.2\_6\_Mar 2012 | A1 |
| 58 | DCS-6210 | V1.00.06 | A1 |
| 59 | DCS-6314 | v1.00.03 | A1 |
| 60 | DCS-6410 | 1.00\_3014 | A1G |
| 61 | DCS-6510 | 1.02 | A1 |
| 62 | DCS-6511 | 1.11.13 | A1 |
| 63 | DCS-6513 | 0.01.00 | A1 |
| 64 | DCS-6615 | 1.01 | A1 |
| 65 | DCS-6616 | 0.01.00 | A1 |
| 66 | DCS-6620 | 1.06 | A3 |
| 67 | DCS-6620G | 1.05 | A4 |
| 68 | DCS-6815 | 1.01 | A1 |
| 69 | DCS-6815 B1 | 0.01.00 | B1 |
| 70 | DCS-6817 | 1.01 | A1 |
| 71 | DCS-6817 B1 | 0.01.00 | B1 |
| 72 | DCS-6818 | 1.01 | A1 |
| 73 | DCS-6818 B1 | 0.01.00 | B1 |
| 74 | DCS-6915 | v1.00.00\_Oct\_02\_2012 | A1 |
| 75 | DCS-7010L | 0.01.05 | A1 |
| 76 | DCS-7110 | 1.0 | A1 |
| 77 | DCS-7410 | 1.00\_3710 | A1 |
| 78 | DCS-7413 | V1.00.02 | A1 |
| 79 | DCS-7513 | 0.01.00 | A1 |
| 80 | DCS-7510 | 1.00\_3909 | A1G |
| 81 | DVS-210-1 | 1.00.01 | A1 |
| 82 | DVS-310-1 | 1.02 | A1 |
| 83 | DVS-V310-4 | 1.00 | A1 |