

|  |  |
| --- | --- |
| **Software Version:** | 1.6.8 |
| **Prom Code Version:** | 4.0 |
| **Published Date:** | 2015/06/17 |

**Content:**

[Revision History and System Requirement: 2](#_Toc228273642)

[New Features: 2](#_Toc228273646)

[Problems Fixed: 2](#_Toc228273649)

[Known Issues: 2](#_Toc228273650)

[Related Documentation: 2](#_Toc219089682)

# Revision History and System Requirement:

|  |  |  |  |
| --- | --- | --- | --- |
| **Firmware Version** | **Date** | **Model** | **Hardware Version** |
| 1.6.8 | 2015/06/17 | DCS-100/210/220/230 | N/A |

# New Features:

|  |  |
| --- | --- |
| **Firmware Version** | **New Features** |
| 1.6.8 | Support new IP camera and new FW:   1. DCS-4602EV(FW V0.02.00) 2. DCS-4802E (Copy from DCS-4602EV) 3. DCS-4201(FW V0.02.00) 4. DCS-6513 (upgrade FW to v1.02) |

# Problems Fixed:

|  |  |
| --- | --- |
| **Firmware Version** | **Problems Fixed** |
| 1.6.8 | N/A |

# Known Issues:

|  |  |
| --- | --- |
| **Firmware Version** | **Known Issues** |
| 1.6.8 | N/A |

# Related Documentation:

# Note:

DP 1.6.8 is only compatible with DCS-100/210/220/230. For DCS-100 v4.0 and DVC 2.0, please use DP v2.0.0 and above version.



|  |  |
| --- | --- |
| **Software Version:** | 1.6.7 |
| **Prom Code Version:** | 3.13.0 |
| **Published Date:** | 2015/05/20 |

**Content:**

[Revision History and System Requirement: 2](#_Toc228273642)

[New Features: 2](#_Toc228273646)

[Problems Fixed: 2](#_Toc228273649)

[Known Issues: 2](#_Toc228273650)

[Related Documentation: 2](#_Toc219089682)

# Revision History and System Requirement:

|  |  |  |  |
| --- | --- | --- | --- |
| **Firmware Version** | **Date** | **Model** | **Hardware Version** |
| 1.6.7 | 2015/05/20 | DCS-100/210/220/230 | N/A |

# New Features:

|  |  |
| --- | --- |
| **Firmware Version** | **New Features** |
| 1.6.7 | 1. Support new IP camera of DCS-1201 (FW:V0.00.01)  2. Support new IP camera of DCS-4701E (FW: V0.00.02) |

# Problems Fixed:

|  |  |
| --- | --- |
| **Firmware Version** | **Problems Fixed** |
| 1.6.7 | N/A |

# Known Issues:

|  |  |
| --- | --- |
| **Firmware Version** | **Known Issues** |
| 1.6.7 | N/A |

# Related Documentation:

# Note:

DP 1.6.7 is only compatible with DCS-100/210/220/230. For DCS-100 v4.0 and DVC 2.0, please use DP v2.0.0 and above version.



|  |  |
| --- | --- |
| **Software Version:** | 1.6.6 |
| **Prom Code Version:** | 3.12.0 |
| **Published Date:** | 2015/05/05 |

**Content:**

[Revision History and System Requirement: 2](#_Toc228273642)

[New Features: 2](#_Toc228273646)

[Problems Fixed: 3](#_Toc228273649)

[Known Issues: 3](#_Toc228273650)

[Related Documentation: 3](#_Toc219089682)

# Revision History and System Requirement:

|  |  |  |  |
| --- | --- | --- | --- |
| **Firmware Version** | **Date** | **Model** | **Hardware Version** |
| 1.6.6 | 2015/03/06 | DCS-100/210/220/230 | N/A |

# New Features:

|  |  |
| --- | --- |
| **Firmware Version** | **New Features** |
| 1.6.6 | Support DCS-7518 (FW:1.00) IP camera. |

# Problems Fixed:

|  |  |
| --- | --- |
| **Firmware Version** | **Problems Fixed** |
| 1.6.6 | Fix DCS-2310LB1 incorrect parameter setting when using auto-search function |

# Known Issues:

|  |  |
| --- | --- |
| **Firmware Version** | **Known Issues** |
| 1.6.6 | DCS-7518:  1. Can not search the camera by UPnP. (Camera firmware issue)  2. Talk function will fail with G.711 a-law. (Camera firmware issue)  3. Camera video parameter of contrast will fail when set up to 9. (Camera firmware issue)  4. The list of resolution and framerate is not synchronized with camera web. (Camera firmware issue) |

# Related Documentation:

# Note:

DP 1.6.6 is only compatible with DCS-100/210/220/230. For DCS-100 v4.0 and DVC 2.0, please use DP v2.0.0 and above version.



|  |  |
| --- | --- |
| **Software Version:** | 1.6.2 |
| **Prom Code Version:** | 3.8.0 |
| **Published Date:** | 2014/10/07 |

**Content:**

[Revision History and System Requirement: 2](#_Toc228273642)

[New Features: 2](#_Toc228273646)

[Problems Fixed: 3](#_Toc228273649)

[Known Issues: 3](#_Toc228273650)

[Related Documentation: 3](#_Toc219089682)

# Revision History and System Requirement:

|  |  |  |  |
| --- | --- | --- | --- |
| **Firmware Version** | **Date** | **Model** | **Hardware Version** |
| 1.6.2 | 2014/10/07 | DCS-100/210/220/230 | N/A |

# New Features:

|  |  |
| --- | --- |
| **Firmware Version** | **New Features** |
| 1.6.2 | **New Camera Supported**  DCS-5222LB1 (FW: 2.01.05)  DCS-5222LB2 (certificate by DCS-5222LB1 (FW: 2.01.05))  DCS-2230L (FW 0.03.00)  DCS-2210L (certificate by DCS-2230L (FW 0.03.00))  DCS-2103 B1 (certificate by DCS-2132L B1 (FW: v2.00.05)) |

# Problems Fixed:

|  |  |
| --- | --- |
| **Firmware Version** | **Problems Fixed** |
| 1.6.2 | n/a |

# Known Issues:

|  |  |
| --- | --- |
| **Firmware Version** | **Known Issues** |
| 1.6.2 | DCS-2230L  1. Talk function is invalid.(Camera firmware issue) |

# Related Documentation:

# Note:

DP 1.6.2 is only compatible with DCS-100/210/220/230. For DCS-100 v4.0 and DVC 2.0, please use DP v2.0.0 and above version.



|  |  |
| --- | --- |
| **Software Version:** | 1.6.1 |
| **Prom Code Version:** | 3.7.0 |
| **Published Date:** | 2014/9/17 |

**Content:**

[Revision History and System Requirement: 2](#_Toc228273642)

[New Features: 2](#_Toc228273646)

[Problems Fixed: 3](#_Toc228273649)

[Known Issues: 3](#_Toc228273650)

[Related Documentation: 3](#_Toc219089682)

# Revision History and System Requirement:

|  |  |  |  |
| --- | --- | --- | --- |
| **Firmware Version** | **Date** | **Model** | **Hardware Version** |
| 1.6.1 | 2014/9/17 | DCS-100/210/220/230 | N/A |

# New Features:

|  |  |
| --- | --- |
| **Firmware Version** | **New Features** |
| 1.6.1 | **1. New Camera Supported**  DCS-2310LB1 (FW: v0.03.00)  DCS-6116 (FW: V1.20)  DCS-6915B1 (certificate by DCS-6915A1 (FW: 1.00.10))  DCS-3010 (FW: v1.12.07)  2. Change “Super Model” name to “Universal Model” name in camera list |

# Problems Fixed:

|  |  |
| --- | --- |
| **Firmware Version** | **Problems Fixed** |
| 1.6.1 | n/a |

# Known Issues:

|  |  |
| --- | --- |
| **Firmware Version** | **Known Issues** |
| 1.6.1 | DCS-2310LB1  1. Control mode of resolution, frame rate, bitrate cannot be changed under H.264  format. (Camera firmware issue)  2. The name of this camera in search window will show as DCS-2310L. (Camera  firmware issue)  DCS-6116  1. Resolution is not synchronized with camera web. (Camera firmware issue)  2. Cannot setup from 13fps to 25fps. (Camera firmware issue)  3. Cannot setup resolution under 720x480. (Camera firmware issue)  DCS-3010  1. Stream may disconnect and motion may not be triggered when setting to  maximum resolution due to camera limited performance. (Camera firmware issue) |

# Related Documentation:

# Note:

DP 1.6.1 is only compatible with DCS-100/210/220/230. For DCS-100 v4.x, DCS-210/220/230 2.x and DCS-250 V1.x above versions, please use DP v2.0.0 and above version.



|  |  |
| --- | --- |
| **Software Version:** | 1.6.0 |
| **Prom Code Version:** | 3.6.0 |
| **Published Date:** | 2014/8/18 |

**Content:**

[Revision History and System Requirement: 2](file:///D:\Steven%20Ku\友訊科技\數位家庭產品處\產品\廠商資料\NUUO%20京晨資訊\委託開發\軟體\Device%20Pack\Formal%20Release%20Notes\D-Link_Device_pack_Release%20Note_V1.6.0_20140818.docx#_Toc228273642)

[New Features: 2](file:///D:\Steven%20Ku\友訊科技\數位家庭產品處\產品\廠商資料\NUUO%20京晨資訊\委託開發\軟體\Device%20Pack\Formal%20Release%20Notes\D-Link_Device_pack_Release%20Note_V1.6.0_20140818.docx#_Toc228273646)

[Problems Fixed: 3](file:///D:\Steven%20Ku\友訊科技\數位家庭產品處\產品\廠商資料\NUUO%20京晨資訊\委託開發\軟體\Device%20Pack\Formal%20Release%20Notes\D-Link_Device_pack_Release%20Note_V1.6.0_20140818.docx#_Toc228273649)

[Known Issues: 3](file:///D:\Steven%20Ku\友訊科技\數位家庭產品處\產品\廠商資料\NUUO%20京晨資訊\委託開發\軟體\Device%20Pack\Formal%20Release%20Notes\D-Link_Device_pack_Release%20Note_V1.6.0_20140818.docx#_Toc228273650)

[Related Documentation: 3](file:///D:\Steven%20Ku\友訊科技\數位家庭產品處\產品\廠商資料\NUUO%20京晨資訊\委託開發\軟體\Device%20Pack\Formal%20Release%20Notes\D-Link_Device_pack_Release%20Note_V1.6.0_20140818.docx#_Toc219089682)

# Revision History and System Requirement:

|  |  |  |  |
| --- | --- | --- | --- |
| **Firmware Version** | **Date** | **Model** | **Hardware Version** |
| 1.6.0 | 2014/8/18 | DCS-100/210/220/230 | N/A |

# New Features:

|  |  |
| --- | --- |
| **Firmware Version** | **New Features** |
| 1.6.0 | **New Camera Supported**  DCS-6314 (multi-stream FW: V1.00.00)  DCS-7010L (G.711 support FW: v1.03.07)  DCS-6517 (FW: V0.00.07)  DCS-7517 (certificate by DCS-6517 FW: V0.00.07)  DCS-6112 (multi-stream FW: v2.10.02)  DCS-6113 (certificate by DCS-6112) |

# Problems Fixed:

|  |  |
| --- | --- |
| **Firmware Version** | **Problems Fixed** |
| 1.6.0 | n/a |

# Known Issues:

|  |  |
| --- | --- |
| **Firmware Version** | **Known Issues** |
| 1.6.0 | DCS-6112/DCS-6113 (camera issues)  1.The camera with highest quality and MJPEG format is unable to achieve 30 fps  2.The audio talk is not supported |

# Related Documentation:

# Note:

DP 1.6.0 is only compatible with DCS-100/210/220/230. For DCS-100 v4.x, DCS-210/220/230 2.x and DCS-250 V1.x above versions, please use DP v2.0.0 and above version.



|  |  |
| --- | --- |
| **Software Version:** | 1.5.8 |
| **Prom Code Version:** | 3.4.0 |
| **Published Date:** | 2014/09/02 |

**Content:**

[Revision History and System Requirement: 2](#_Toc228273642)

[New Features: 2](#_Toc228273646)

[Problems Fixed: 3](#_Toc228273649)

[Known Issues: 3](#_Toc228273650)

[Related Documentation: 3](#_Toc219089682)

# Revision History and System Requirement:

|  |  |  |  |
| --- | --- | --- | --- |
| **Firmware Version** | **Date** | **Model** | **Hardware Version** |
| 1.5.8 | 2014/6/6 | DCS-100/210/220/230 | N/A |

# New Features:

|  |  |
| --- | --- |
| **Firmware Version** | **New Features** |
| 1.5.8 | **New Camera Supported**  DCS-6513 (FW: V1.01.02) (FW upgrade)  DCS-6045L (FW: V1.00b3)  DCS-942LB1 (FW:V2.00\_3815) |

# Problems Fixed:

|  |  |
| --- | --- |
| **Firmware Version** | **Problems Fixed** |
| 1.5.8 | [DBG14030171] D-ViewCam SW couldn't stop DUT auto-pan. |

# Known Issues:

|  |  |
| --- | --- |
| **Firmware Version** | **Known Issues** |
| 1.5.8 | n/a |

# Related Documentation:

# Note:



|  |  |
| --- | --- |
| **Software Version:** | 1.5.7 |
| **Prom Code Version:** | 3.3.0 |
| **Published Date:** | 2014/06/23 |

**Content:**

[Revision History and System Requirement: 2](#_Toc228273642)

[New Features: 2](#_Toc228273646)

[Problems Fixed: 3](#_Toc228273649)

[Known Issues: 3](#_Toc228273650)

[Related Documentation: 3](#_Toc219089682)

# Revision History and System Requirement:

|  |  |  |  |
| --- | --- | --- | --- |
| **Firmware Version** | **Date** | **Model** | **Hardware Version** |
| 1.5.7 | 2014/06/23 | DCS-100/210/220/230 | N/A |

# New Features:

|  |  |
| --- | --- |
| **Firmware Version** | **New Features** |
| 1.5.7 | **New Camera Supported**  DCS-930LB1 (FW:v2.00 b1)  DCS-932LB1 (certificate DCS-930LB1, FW:v2.00 b1)  DCS-6112B1 (FW v3.00.00)  DCS-6113B1 (certificate DCS-6112B1, FW: v3.00.00)  DCS-6113VB1 (certificate DCS-6112B1, FW: v3.00.00) |

# Problems Fixed:

|  |  |
| --- | --- |
| **Firmware Version** | **Problems Fixed** |
| 1.5.7 | n/a |

# Known Issues:

|  |  |
| --- | --- |
| **Firmware Version** | **Known Issues** |
| 1.5.7 | **DCS-930LB1**  Auto detection is not supported. (camera firmware issue)  **DCS-6112B1**  The camera with highest quality and MJPEG format is unable to achieve 30  fps.(camera firmware issue)  Audio out is not supported. (camera firmware issue) |

# Related Documentation:

# Note:



|  |  |
| --- | --- |
| **Software Version:** | 1.5.6 |
| **Prom Code Version:** | 3.2.0 |
| **Published Date:** | 2014/06/20 |

**Content:**

[Revision History and System Requirement: 2](#_Toc228273642)

[New Features: 2](#_Toc228273646)

[Problems Fixed: 3](#_Toc228273649)

[Known Issues: 3](#_Toc228273650)

[Related Documentation: 3](#_Toc219089682)

# Revision History and System Requirement:

|  |  |  |  |
| --- | --- | --- | --- |
| **Firmware Version** | **Date** | **Model** | **Hardware Version** |
| 1.5.6 | 2014/4/23 | DCS-100/210/220/230 | N/A |

# New Features:

|  |  |
| --- | --- |
| **Firmware Version** | **New Features** |
| 1.5.6 | **Camera FW upgrade**  DCS-2132LB1 (FW v2.00.05)  DCS-3112 (FW v1.11.01)  DCS-3010 (v1.11.00) support dual stream  DCS-3714 (FW v1.00.00)  DCS-6115 (FW: V0.09.00)  **New Camera Supported**  DCS-7000L (FW:v0.09.00) |

# Problems Fixed:

|  |  |
| --- | --- |
| **Firmware Version** | **Problems Fixed** |
| 1.5.6 | n/a |

# Known Issues:

|  |  |
| --- | --- |
| **Firmware Version** | **Known Issues** |
| 1.5.6 | **DCS-2132LB1**  Motion detection may not trigger continuously within short period of time. (camera firmware issue)  **DCS-3112**   * With MPEG4 format, the resolution list is not synchronized with the one on camera’s web. (camera firmware issue). * Under multi stream function, low and min stream cannot reach 500 kbps and 100 kbps.   **DCS-3010**   * Motion detection is highly possible out of function after setting camera parameter. * Setting bitrate to 8000kbps will fail. * High resolution makes video slow motion.   **DCS-3714**   * The camera with highest quality and resolution is unable to achieve 30 fps. (camera firmware issue)   **DCS-6115**   * The camera with highest quality and MJPEG format is unable to achieve 30 fps and audio will stutter. (camera firmware issue)   **DCS-7000L**   * The camera with highest quality/resolution and MJPEG format is unable to achieve 30 fps. (camera firmware issue) * The parameters of the camera are not configurable with H.264 format. (camera firmware issue) * The format of the camera is not configurable from MJPEG to H.264. (camera firmware issue) * The list of camera format MPEG4 isn’t synchronized with the one on camera’s web. If user sets camera format to MPEG4, camera will crash. (camera firmware issue) * Motion detection may not trigger continuously. (camera firmware issue) |

# Related Documentation:

# Note:



|  |  |
| --- | --- |
| **Software Version:** | 1.5.5 |
| **Prom Code Version:** | 3.0.0 |
| **Published Date:** | 2014/2/14 |

**Content:**

[Revision History and System Requirement: 2](#_Toc228273642)

[New Features: 2](#_Toc228273646)

[Problems Fixed: 3](#_Toc228273649)

[Known Issues: 3](#_Toc228273650)

[Related Documentation: 3](#_Toc219089682)

# Revision History and System Requirement:

|  |  |  |  |
| --- | --- | --- | --- |
| **Firmware Version** | **Date** | **Model** | **Hardware Version** |
| 1.5.5 | 2014/2/14 | DCS-100/210/220/230 | N/A |

# New Features:

|  |  |
| --- | --- |
| **Firmware Version** | **New Features** |
| 1.5.5 | Camera FW upgrade:  DCS-3010 (from v1.00.05 to v1.11.00)  Support new camera:  DCS-3714 (FW : 0.01.00\_test)  DCS-6045L (v0.99\_b3)  DCS-5222LB1 (FW : 2.00.05 2014.1.3) |

# Problems Fixed:

|  |  |
| --- | --- |
| **Firmware Version** | **Problems Fixed** |
| 1.5.5 | n/a |

# Known Issues:

|  |  |
| --- | --- |
| **Firmware Version** | **Known Issues** |
| 1.5.5 | **DCS-3010**   1. Motion detection may fail after setting camera parameter. (camera firmware issue) 2. Camera may not work when setup bitrate to 8000kbps. (camera firmware issue) 3. Not support dual stream. 4. The live view may delay when setup high resolution. (camera firmware issue)   **DCS-5222LB1**   1. Not support talk. (camera firmware issue) 2. Not support preset. (camera firmware issue) 3. Direction of PTZ is opposite. (camera firmware issue) 4. The live view may delay when setup high resolution. (camera firmware issue)   **DCS-3714**   1. Not support 8M bitrate. (camera firmware issue)   **DCS-6045L**   1. It may need to reboot again after a period of time. (camera firmware issue) |

# Related Documentation:

# Note: