ALPHA DAP-3520 D-VIEW Release Note v1.01-r14

Firmware: 1.01r020
Build Number : 95l4
Hardware: DAP3520
D-View:  v1.01r14
Date:  June 26, 2009
Problems Resolved:
1. Fixed bugs about the sequence of the pages in the DHCP Server settings.
2. Fixed bugs about the displaying error while the Static Pool Settings is selected in the DHCP Server settings.
3. Fixed bugs about the Performance settings and the Device Information (Wireless band is 2.4G).
4. Fixed bugs about the Performance settings and the Device Information (Wireless band is 5G).
5. Fixed bugs about the displaying of System Name and Location in the Administrator Settings.

ALPHA DAP-3520 D-VIEW Release Note v1.01-r13

Firmware: 1.01r020
Build Number : 95l4
Hardware: DAP3520
D-View:  v1.01r13
Date:  June 26, 2009
Problems Resolved:
1.	Fixed bugs about the controls’ sequence of Tab Order in function or page of wireless settings.
2.	Fixed bugs about the un-closable displaying dialog when Priority class is set and Add button is clicked. The result is the displaying dialog is cancelled and the information shows up in Status bar.
3.	Fixed bugs about the warning message while the NTP Server's IP address is null.

ALPHA DAP-3520 D-VIEW Release Note v1.01-r12

Firmware: 1.01r020
Build Number : 95l4
Hardware: DAP3520
D-View:  v1.01r12
Date:  June 25, 2009
Problems Resolved:
1. Fixed bugs about the MAC address in the mapping list from changeable state to unchangeble state while clicking.
2. Fixed bugs to show up the Host Name parameter in the Current DHCP Static Pools.
3. Fixed bugs about the IP displaying while making changes about the IP settings.

ALPHA DAP-3520 D-VIEW Release Note v1.01-r11

Firmware: 1.01r020
Build Number : 95l4
Hardware: DAP3520
D-View:  v1.01r11
Date:  June,22, 2009
Problems Resolved:
1: Fixed bugs about SysLog from invalid state to valid state..

ALPHA DAP-3520 D-VIEW Release Note v1.01-r10

Firmware: 1.01r020
Build Number : 95l4
Hardware: DAP3520
D-View:  v1.01r10
Date:  June,02, 2009
Problems Resolved:
1: Fixed bugs about wirless channel list.
2: Fixed bugs when change WPA-EAP to WEP.

ALPHA DAP-3520 D-VIEW Release Note v1.01-r09

Firmware: 1.01r020
Build Number : 95l4
Hardware: DAP3520
D-View:  v1.01r09
Date:  May 27, 2009
Problems Resolved:

1.	Add data Special for JP
2.	Modify Wireless Mode when open system,share key enabled,and so on.

ALPHA DAP-3520 D-VIEW Release Note v1.00-r08

Firmware: 1.00r016
Build Number : 93hg
Hardware: DAP3520
D-View:  v1.00r08
Date:  March 27, 2009
Problems Resolved:

3.	d-view5.1 platform,in main form,there is the information of DLSNMP++;
4.	The Limit Administrator VID value should be 1~4094.
5.	When choose 5GHz band and 149 channel, the channel width should be changeable
6.	When coutry code is JP, there are something wrong about WPA authentication.
7.	There are something error about Auto Channel Scan and Channel Width when we choose AP Client mode.
8.	The IP assigned of the Dynamic Pool should be valid all the time.
Enhancements:

Firmware: 1.00r015
Build Number : 939c
Hardware: DAP3520
D-View:  v1.00r07
Date:  March 23, 2009
Problems Resolved:

9.	When ap mode is wireless client, Link Integrity is gray
10.	when la nip = static ip,will pop warning message
11.	when country is KR,the channel width is the only item 20MHZ
Enhancements:

Firmware: 1.00r014
Build Number : 939c
Hardware: DAP3520
D-View:  v1.00r06
Date:  March 11, 2009
Problems Resolved:

12.	Add the function of Link Integrity.
13.	When country is JP and GB,and the band is 5Ghz,ap mode is the two items :access point and wireless client
14.	In wireless page,the error message when refresh.
15.	There is no check-all-pane square in Wireless Intrusion Protection page.
Enhancements:

ALPHA DAP-3520 D-VIEW Release Note v1.00-r04
Firmware: 1.00r010
Build Number : 92di
Hardware: DAP3520
D-View:  v1.00r04
Date:  Feb 16, 2009
Problems Resolved:

16.	The problem about the description in device.
17.	The LED in the main page should show the same just as the AP itself.
18.	When WISP mode is choosen, the BSSID of the remote APs are all zero.
19.	When choose "Manual" as connect mode, there should show two buttons "Connect" and "Disconnect".
20.	The function of the smtp should be removed.
21.	The Beacon Interval and DTIM show blank in web page.
22.	When Wireless Client mode or WISP Client Router mode is choosen, The ShortGI shows "Disable" in web page, but it's shows different in console and D-View module.
23.	Home \Internet Connection: There are some spell mistakes when a warning message is shown.
24.	When choose clone MAC Address and set apply, there is a warning message.

ALPHA DAP-3520 D-VIEW Release Note v1.00-r03
Firmware: 1.00r008
Build Number : 91ck
Hardware: DAP3520
D-View:  v1.00r03
Date:  Feb 4, 2009
Problems Resolved:

1. There is some function errors about the default gateway setting
2. When change the authentication method in some way, there shows some error information.
3. In D-View module, The channel should be changed to be the same with the remote AP when Wireless Client or WISP Client Router mode is choosen, just like in the web page.
4. When set Primary SSID as PSK authenticaton, it shows the EAP in Multi-SSID page
5. When enable DHCP Server function and STAs get IP address from AP, the Current IP Mapping List show nothing about client information
6. When VLAN Status is disabled, the VLAN Name can not be modified in anytime. But when click "Edit" button in VLAN List page under the background of VLAN disabled, the VLAN Status should be changed to Enable automatically.
7. When WISP Client Router mode is choosen, there would be some function fails if the Internet Connection Type is PPPoE.
8. When WISP Client Router mode is choosen and set Internet Connection Type to PPTP, it failed to take effect.
9.When WISP Client Router mode is choosen and Internet Connection Type is Static IP, the MTU value can be saved only as 1400.
10. Home \ Internet connection: in this page, click Cancel, it did not take effect.
11. 1.Set band to 5GHz, ap mode to wireless client or WISP client router, the mac source will show blank, the mac address will show 00000000..change band from 5GHz to 2.4GHz, the problem exist all the same.
12. Change ap mode from client mode(2 modes) to WDS mode(2 modes), the button of Scan should be gray.
13.
Enhancements: 

ALPHA DAP-3520 D-VIEW Release Note v1.00-r02
Firmware: 1.00r008
Build Number : 91ck
Hardware: DAP3520
D-View:  v1.00r02
Date:  Jan 22, 2009
Problems Resolved:

1.Fixed the bugs on the bug tracking.

Enhancements: 
1.The pictures and the led control;
2.The MTU Setting;
3.The status of QOS

ALPHA DAP-3520 D-VIEW Release Note v1.00-r01
Firmware: 1.00r007
Build Number : 91ck
Hardware: DAP3520
D-View:  v1.00r01
Date:  Jan 13, 2009
Problems Resolved:
Enhancements: 
New Project