

|  |  |
| --- | --- |
| **Firmware Version:** | 1.01r006 |
|  |  |
| **Published Date:** | 2024/04/23 |
|  |  |

**Content:**

[Upgrading Instructions: 2](#_Toc273021139)

[Upgrading by using Web-UI 2](#_Toc273021140)

[New Features: 2](#_Toc273021141)

[Changes of MIB & D-View Module: 2](#_Toc273021142)

[Problems Fixed: 3](#_Toc273021143)

[Known Issues: 3](#_Toc273021144)

[Related Documentation: 3](#_Toc273021145)

Revision History and System Requirement:

|  |  |  |  |
| --- | --- | --- | --- |
| **Firmware Version** | **Date** | **Model** | **Hardware Version** |
|  |  |  |  |

# Upgrading Instructions:

D-Link AP supports firmware upgrading via Web-UI. You may download the firmware from D-Link web site <http://tsd.dlink.com.tw>.

Please also

1. Make sure your DAP-X3060 has to manually assign a valid static IPv4 address or get a valid IPv4 address from DHCP server before upgrade FW.
2. Do not power off your DAP-X3060 when FW upgrading.

## Upgrading by using Web-UI

1. Connect a work station to the LAN port of Access Point.
2. Open the web browser of work station and entering the IP address of the AP. The system default IP address setting is dynamic ip, and you can enter <http://dapx3060.local> to login, if it cannot get ip address from DHCP server, it’s ip address will back to 192.168.0.50.
3. Enter administrator’s username and password, user name and password are “admin” by default.

To update the AP's firmware, click **Maintenance > Firmware and SSL Certification Upload**

# New Features:

1. Enable DFS channel for FCC & IC
2. Support click through feature in standalone moe

# Changes of MIB & D-View Module:

None

# Problems Fixed:

|  |  |
| --- | --- |
| **Firmware Version** | **Problems Fixed** |
| V1.01 | 1. [DBG] Fix Bad Gateway issue
2. [D-Track]Fix WMM for multi SSID1~7 can be selected Enable or Disable
 |

# Known Issues:

|  |  |
| --- | --- |
| **Firmware Version** | **Known Issues** |
| V1.01 | None |

# Related Documentation:

DAP-X3060 user manual v1.00