

|  |  |
| --- | --- |
| **Software Version:** | 1.4.3.1 |
| **Prom Code Version:** |  |
| **Published Date:** | 2012/11/09 |

**Content:**

[Revision History and System Requirement: 2](#_Toc228273642)

[New Features: 2](#_Toc228273646)

[Problems Fixed: 3](#_Toc228273649)

[Known Issues: 3](#_Toc228273650)

[Related Documentation: 3](#_Toc219089682)

# Revision History and System Requirement:

|  |  |  |  |
| --- | --- | --- | --- |
| **Firmware Version** | **Date** | **Model** | **Hardware Version** |
| V1.4.3.1 | 2012/07/11 | DCS-100/210/220/230 | N/A |
|  |  |  |  |
|  |  |  |  |

# New Features:

|  |  |
| --- | --- |
| **Firmware Version** | **New Features** |
| 1.4.3.1 | 1. Add camera: DCS-2332L |

# Problems Fixed:

|  |  |
| --- | --- |
| **Firmware Version** | **Problems Fixed** |
| 1.4.3.1 | 1. Fixed DCS-2132L would cause D-ViewCam shut down issue 2. Fixed live view bug for DCS-930/932L/930L/910/920 (**DBG12060162)** |
|  |  |

# Known Issues:

|  |  |
| --- | --- |
| **Firmware Version** | **Known Issues** |

# Related Documentation:

N/A

# Note:

**HW Support List for Device Pack 1.4.3.1:**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Device  Name** | **Final FW** | **Device  Name** | **Final FW** | **Device  Name** | **Final FW** |
| DCS-910 | 1.04\_build\_5 | DCS-920 | 1.04\_build\_5 | DCS-930 | 1.00 build 2 |
| DCS-930L | 1.00 build 2 | DCS-932 | 1.00 | DCS-940L | 1 |
| DCS-2103 |  | DCS-932L | 1.00 | DCS-942L | 1 |
| DCS-2210 | 0.02.00 | DCS-2310L |  | DCS-1100 | 1.02\_3522 |
| DCS-2120 | 1.04\_3227 | DCS-3110 | 1.02 | DCS-1100L | 1.03\_4130 |
| DCS-2120(TW) | 2.01tw | DCS-3112 |  | DCS-1130 | 1.02\_3522 |
| DCS-2121 | 1.04\_3227 | DCS-3410 | 1.01\_2812 | DCS-1130L | 1.03\_4130 |
| DCS-2130 |  | DCS-3411 | 1.02\_4125 | DCS-2102 | 1.04\_3227 |
| DCS-2132L | 0.02.00 | DCS-3710 | 1.00 | DCS-5220Bx | 2.00 |
| DCS-2230 | 0.02.00 | DCS-3710 B1 | 0.02.00 | DCS-5220(TW) | 2.00tw |
| DCS-3415 | 1.00 | DCS-3715 | 1.00 | DCS-5222L |  |
| DCS-3420 | 1.03 | DCS-3716 |  | DCS-5230 | 1.02\_4317 |
| DCS-3430 | 1.02\_4125 | DCS-5211L |  | DCS-5230L | 1.02\_4317 |
| DCS-5300G | 2.05 | DCS-5220Ax | 1.05 | DCS-5300 | 1.06 |
| DCS-5605 | 1.01\_4126 | DCS-6112 | X | DCS-6615 | 1.01 |
| DCS-5610 | 1.01 | DCS-6113 | X | DCS-6616 | 0.01.00 |
| DCS-5635 | 1.01\_4126 | DCS-6112V | X | DCS-6620 | 1.06 |
| DCS-6010L | 0.01.13 | DCS-6113V | X | DCS-6620G | 1.05 |
| DCS-6110 | 1.00 | DCS-6410 | 1.00\_3014 | DCS-6815 | 1.01 |
| DCS-6510 | 1.02 | DCS-6818 | 1.01 | DCS-6815 B1 | 0.01.00 |
| DCS-6511 | 0.08 | DCS-6818 B1 | 0.01.00 | DCS-6817 | 1.01 |
| DCS-6817 B1 | 0.01.00 | DVS-210-1 | 1.00.01 | DCS-7010L | 0.01.05 |
| DCS-7410 | 1.00\_3710 | DVS-310-1 | 1.02 | DCS-7110 | 1.0 |
| DCS-7413 | 0.01.00 | DCS-7513 | 0.01.00 | DCS-7510 | 1.00\_3909 |
| DVS-V310-4 | 1.00 | DCS-2332L | 0.01.02 (refer 2132L CGI) |  |  |