### DNS-327L Firmware Release Notes

**Version: 1.03**

**Hardware: A1**

**Date: 2014/07/22**

**New Features:**

None

**Enhancements:**

None

**Problems Resolved:**

[Security] The port parameter of login\_mgr.cgi has been fixed.

[Multimedia] Missing Multimedia Share Folder List is fixed

[DDNS] The free www.DynDNS.org service is no longer offered and has been removed.

-------------------------------------------

**Version: 1.02**

**Hardware: A1**

**Date: 2014/04/22**

**New Features:**

None

**Enhancements:**

None

**Problems Resolved:**

1. Fixed OpenSSL heart bleed issue

-------------------------------------------

**Version: 1.01**

**Hardware: A1**

**Date: 2013/12/13**

**New Features:**

1. Add Google Drive sync function
2. Add System services page
3. Register a mydlink account through NAS Web GUI
4. Xunlei add-on is integrated on DNS-327L (for CN model)

**Enhancements:**

1. [My surveillance]

. Support camera models DCS-7010L/DCS-2310L/DCS-2332L/DCS-6010L

. Support camera models DCS-2132L/ DCS-931L/ DCS-933L/ DCS-5010L/ DCS-5020L

. Supports generic D-Link model which complies NIPCA protocol

. Enhance camera list UI in "Camera setup", "Audio and video" and "Recording Setup"

1. [Multimedia] Enhance Contents Aggregation (pause/resume, show current processing file name, how many file remains)
2. [Amazon S3] Support multiple upload function
3. [P2P] open P2P function in the new tab
4. [HTTP Download] Length of http download URL limitation from 256 to 1024
5. [Web GUI] Enhance storage space used info at home page
6. [Web GUI] Be able to log-in at NAS by pressing "Enter" on keyboard
7. [System Event] Latest log should appear on top of the list at home page
8. Update media library
9. Enable my surveillance center function in landing page

**Problems Resolved:**

1. Fixed unable to perform RAID migration from single disk to RAID1 disk volume
2. Fixed NAS can't be accessed via the SSL port after SSL port be changed and reboot
3. Fixed web security issue
4. Fixed system configuration cannot import with SAMBA configuration setting issue
5. Fixed accessing FTP files via IE browser security issue
6. Fixed FTP server cannot auto update with DNR-322L issue
7. Fixed P2P service causes CPU 100% loading while downloading torrent files

-------------------------------------------

**Firmware: 1.00**

**Hardware: A1**

**Date: 2013/4/9**

First DNS-327L firmware release.

**New Features:**

None

**Enhancements:**

None

**Problems Resolved:**

None

**Known Issues:**

None