DWL-2700 AP Firmware Release Note

Firmware: v3.20 (v3.20rc157)
Hardware: Rev. B1, B2
Date: Aug 18, 2008 

Problem Resolved:
1.	User will fail to login to the management web UI via IE 7.0 if silverlight was installed.
2.	MSSID will be modified if primary SSID security is set to 802.1x.
3.	When change primary SSID settings, sometimes MSSID will also be changed.

Enhancements:
1.	Add Administration VLAN feature.
2.	Add Primary SSID with VLAN tag.
3.	Add Secondary (backup) Radius Server for WPA (2) Enterprise settings.
4.	Support Priority by SSID.
5.	Support Microsoft NAP feature.
6.	Support IGMP snooping v1/v2.
7.	Add Rogue AP detection function.
8.	Support Acct-Interim-Interval attribute for accounting function.
9.	Add system and wireless sub trap group. User can also enable or disable the
trap categorization.
10.	Support to administrate AP with WLAN (Default enable).
11.	Support four management IP range.
12.	Add CLI command to input SNMP Location.
13.	Add Ping control setting.
14.	Add WMM control on each MSSID.
15.	Support AP Manager II v2.
16.	Support MSSID over WDS.
17.	Support IAPP.
18.	Add wireless station linkup and link down trap.

---------------------- END ----------------------